CDA6530: Project 4 Solution (Fall 2010)



Fig. 1: Compare of theoretic solution and simulation solution for Task #1 (no delay). Simulation result is averaged over 100 simulation runs.



Fig. 2: Simulated I(t) from the first 3 simulation runs (without delay consideration)



Fig. 3: Compare of results of simulation with and without delay consideration